<?xml version="1.0" encoding="utf-8"?>
<String xml:lang="en" xmlns="http://www.epson.com/EpsonNet/Resource/Common/StringInfo/1-0">
	<s id="APP_CAPTION">Epson Firmware Updater</s>
	<s id="APP_LANG">en</s>
	<s id="BUTTON_OK">OK</s>
	<s id="BUTTON_CANCEL">Cancel</s>
	<s id="BUTTON_YES">Yes</s>
	<s id="BUTTON_NO">No</s>
	<s id="BUTTON_CLOSE">Close</s>
	<s id="BUTTON_BACK">&lt;Back(&amp;B)</s>
	<s id="BUTTON_NEXT">Next(&amp;N)&gt;</s>
	<s id="BUTTON_START">Start</s>
	<s id="BUTTON_ABORT">Stop</s>
	<s id="BUTTON_CONTINUE">Continue</s>
	<s id="BUTTON_COMPLETE">Finish</s>
	<s id="BUTTON_PRINTSTATUS">Print Version</s>
	<s id="BUTTON_RETRY">Retry(&amp;R)</s>
	<s id="BUTTON_LOGIN">Login</s>
	<s id="BUTTON_SELECTALL">Select All</s>
	<s id="BUTTON_SELECTCLEAR">Remove All</s>
	<s id="BUTTON_REFRESH">Refresh</s>
	<s id="BUTTON_BROWS">Browse...</s>
	<s id="BUTTON_LISENCE1">Legal Notices...</s>
	<s id="BUTTON_LISENCE2">License Agreement...</s>
	<s id="BUTTON_SAVE">Save as file...</s>
	<s id="BUTTON_ADD">Add...</s>
	<s id="BUTTON_DEL">Delete</s>
	<s id="BUTTON_UP">Up</s>
	<s id="BUTTON_DOWN">Down</s>
	<s id="DLG_CAPTION_LISENCE1">Legal Notices</s>
	<s id="DLG_CAPTION_LISENCE2">License Agreement</s>
	<s id="MENU_OPTION">Options(&amp;O)...</s>
	<s id="MENU_VERSION">About Firmware Updater(&amp;A)...</s>
	<s id="TEXT_BOOTING">Launching the application...</s>
	<s id="TEXT_PREPARING">Preparing for firmware update...</s>
	<s id="TITLE_START">Introduction</s>
	<s id="TEXT_START_1">This software allows you to update the firmware for Epson printers/scanners.</s>
	<s id="TEXT_START_2">To continue, click [Next].\nTo quit this software, click [Cancel].</s>
	<s id="TITLE_LISENCE">Software License Agreement</s>
	<s id="TEXT_LISENCE_1">Read the following software license agreement.</s>
	<s id="TEXT_LISENCE_2">Do you agree to all of the terms in the license agreement?\nIf you agree, select [I agree] and then click [Next].\n</s>
	<s id="RADIO_AGREE">I agree.</s>
	<s id="RADIO_NOTAGREE">I do not agree.</s>
	<s id="SAVEFILE_NAME">Software License Agreement</s>
	<s id="SAVEFILE_FILTER">Text file (*.txt)|*.txt|All file (*.*)|*.*||</s>
	<s id="TITLE_FILESELECT">Select Firmware File</s>
	<s id="TEXT_FILESELECT_1">Click [Browse], select the firmware file, and then click [Next].</s>
	<s id="TEXT_FILESELECT_2">Firmware File:</s>
	<s id="OPENFILE_FILTER">Firmware (*.efu)|*.efu|All file (*.*)|*.*||</s>
	<s id="TITLE_WARNING">Instructions and Precautions for Update</s>
	<s id="TITLE_NW_SEARCHING">Select the Printer</s>
	<s id="TEXT_NW_SEARCHING_1">1. Under Model Name, select the printer(s) you want to update.\n2. Click [Start] to begin updating.</s>
	<s id="TEXT_NW_SEARCHING_2">Firmware File:</s>
	<s id="TEXT_NW_SEARCHING_STATUS_SEARCH">Searching</s>
	<s id="TEXT_NW_SEARCHING_STATUS_READY">Ready</s>
	<s id="TITLE_NW_FIREWALL">Firewall Warning</s>
	<s id="TEXT_NW_FIREWALL_1_WIN1">Windows Firewall software will need to allow the Epson Firmware Updater to proceed with the update. Do you want to continue?\nIf you see a firewall warning message, click [Unblock] or [Allow] to let Epson Firmware Updater to continue.</s>
	<s id="TEXT_NW_FIREWALL_1_WIN2">Firewall or anti-spyware software may display alert messages related to the update.\nIf a Firewall message appears, click [Unblock] or [Allow] to let Epson Firmware Updater continue.</s>
	<s id="TEXT_NW_FIREWALL_1_MAC">Firewall or anti-spyware software may disturb the update.</s>
	<s id="TEXT_NW_FIREWALL_2">Click here for more detailed information.</s>
	<s id="TEXT_UPDATECAUTION_1">\nFor printers designed to use Epson genuine cartridges only: Non-Epson branded or altered Epson cartridges that functioned prior to a firmware update may not continue to function.</s>
	<s id="CHECK_FIREWALL">Allow Access (Windows Firewall only)</s>
	<s id="TEXT_UPDATE_1">Overall Progress:</s>
	<s id="TEXT_UPDATE_2">Current Progress:</s>
	<s id="TEXT_UPDATE_5">Update Printer List:</s>
	<s id="TEXT_UPDATE_8">Detailed Information:</s>
	<s id="CHECK_DONT_CONFIRM_CONTINUE">This dialog will not be displayed again.</s>
	<s id="COLUMN_MODELNAME">Model Name</s>
	<s id="COLUMN_ROUTE">Connection Type</s>
	<s id="COLUMN_ROUTE_LOCAL">USB</s>
	<s id="COLUMN_ROUTE_NETWORK">Network</s>
	<s id="COLUMN_IPADDR">IP Address</s>
	<s id="COLUMN_MACADDR">MAC Address</s>
	<s id="COLUMN_STATUS">Status</s>
	<s id="COLUMN_VERSION">Version</s>
	<s id="COLUMN_SOFTWARE">Software</s>
	<s id="COLUMN_VENDOR">Vendor Name</s>
	<s id="COLUMN_CATEGORY">Category</s>
	<s id="COLUMN_FIRMWARETYPE">Firmware type</s>
	<s id="COLUMN_UPDTAEFILE">Update file</s>
	<s id="COLUMN_CURENTVERSION">Current version</s>
	<s id="COLUMN_PACKAGE">Package</s>
	<s id="COLUMN_FIRMWARE">Firmware</s>
	<s id="COLUMN_OTHER">Others</s>
	<s id="COLUMN_VERSION_SAME">Same version</s>
	<s id="COLUMN_VERSION_UP">New version</s>
	<s id="COLUMN_VERSION_DOWN">Old version</s>
	<s id="COLUMN_VERSION_DISABLE_DOWN">Downgraded (It cannot be updated)</s>
	<s id="COLUMN_VERSION_DISABLE_CUSTOM">Specialized (It cannot be updated)</s>
	<s id="COLUMN_VERSION_DISABLE_RAWPORT">Raw port is disabled (It cannot be updated)</s>
	<s id="COLUMN_VERSION_DISABLE_USING">Printer is busy (It cannot be updated)</s>
	<s id="COLUMN_VERSION_DISABLE_USING_SCANNER">Scanner is busy (It cannot be updated)</s>
	<s id="COLUMN_VERSION_UNKNOWN">Unknown</s>
	<s id="COLUMN_VERSION_NONE">Not Installed</s>
	<s id="STATE_UPDATE">Updating</s>
	<s id="STATE_UPDATE_AUTHENCATING">Confirming printer password.</s>
	<s id="STATE_UPDATE_WAIT_IDLE">Printer ready and standing by.</s>
	<s id="STATE_UPDATE_SENDING">Transmitting firmware file to the printer.</s>
	<s id="STATE_UPDATE_WAIT_UPDATING">Firmware update in progress.</s>
	<s id="STATE_UPDATE_WAIT_UPDATING_WARNING">Do not turn off your product while updating even if its LCD screen turns off or blue.</s>
	<s id="STATE_UPDATE_REBOOTPOLLING">Waiting for the printer to restart.</s>
	<s id="STATE_UPDATE_CHECKVERSION">Firmware version confirmed.</s>
	<s id="STATE_FIRM_SENDED">Transfer complete</s>
	<s id="STATE_SUCCEED">Update successful</s>
	<s id="STATE_SUCCEED_DEFAULT">The firmware update is complete.</s>
	<s id="STATE_SUCCEED_AUTOPOWEROFF">The firmware has been downloaded to your printer.\nWait for the printer to turn off automatically. </s>
	<s id="STATE_SUCCEED_EZ_AUTOPOWEROFF">The firmware has been downloaded to your printer.\nWait for the printer to turn off automatically. </s>
	<s id="STATE_SUCCEED_BIJ_RECOVERY">The firmware has been downloaded to your printer.</s>
	<s id="STATE_SUCCEED_WIFI_DIRECT"></s>
	<s id="STATE_FAILED">Update failed</s>
	<s id="STATE_FAILED_WAIT_IDLE">The printer could not be updated.</s>
	<s id="STATE_FAILED_CAUSE_WAIT_IDLE">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off (disable the Power Off Timer setting in the printer).\n- The printer is busy.\n- A printer error has occurred.</s>
	<s id="STATE_FAILED_SENDING">Failed to send the firmware file to the printer.</s>
	<s id="STATE_FAILED_CAUSE_SENDING">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off (disable the Power Off Timer setting in the printer).\n- The printer is busy.\n- A printer error has occurred.</s>
	<s id="STATE_FAILED_REBOOTPOLLING">Cannot confirm if the printer has restarted.</s>
	<s id="STATE_FAILED_CAUSE_REBOOTPOLLING">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.\n- There was a loss of power to the printer during the firmware update.</s>
	<s id="STATE_FAILED_CHECKVERSION">The printer&apos;s firmware was not updated.</s>
	<s id="STATE_FAILED_CAUSE_CHECKVERSION">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.</s>
	<s id="STATE_FAILED_AUTOSHUTDOWN">- The printer may have turned off if its Power Off Timer setting is enabled.</s>
	<s id="STATE_FAILED_AUTOSHUTDOWN_RESTORE">The Power Off Timer was not restored to its original setting.  </s>
	<s id="STATE_FAILED_AUTOSHUTDOWN_DISABLE">Power Off Timer of the printer has not been invalid.</s>
	<s id="STATE_FAILED_CAUSE_AUTOSHUTDOWN_DISABLE">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.</s>
	<s id="ERR_EZ_NOTFOUND">The printer was not detected.</s>
	<s id="ERR_EZ_CAUSE_NOTFOUND">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.</s>
	<s id="ERR_EZ_NOTTARGET">The firmware has not been updated because it is not for the printer connected.</s>
	<s id="ERR_EZ_CUSTOMFIRM">The firmware has not been updated because exclusive firmware has been applied.</s>
	<s id="ERR_EZ_DOWNGRADE">The firmware does not need to be updated because the latest version of firmware has been applied.</s>
	<s id="ERR_EZ_DISABLEDRAWPORT">The firmware has not been updated because the raw port is disabled.</s>
	<s id="STATE_CANCELING">Canceling update</s>
	<s id="STATE_CANCELING_DETAIL">The Power Off Timer will be returned to its original settings.</s>
	<s id="STATE_CANCELING_DETAIL_SCANNER">The Power Off Timer will be returned to its original settings.</s>
	<s id="STATE_CANCELED">Cancel update</s>
	<s id="STATE_CANCELED_DETAIL">The update was canceled by the user.</s>
	<s id="STATE_WAITING">The update is standing by</s>
	<s id="STATE_WAITING_DETAIL">Waiting to complete update for other printers.</s>
	<s id="DLG_PRINTING_TEXT_1">Printing information on a current version...</s>
	<s id="DLG_CAPTION_SOFTWARE">Software Information</s>
	<s id="DLG_CAPTION_PASSWORD">Password</s>
	<s id="GROUP_LOGIN">Printer Logon</s>
	<s id="GROUP_LOGIN_MSG1">Enter the current administrator password.</s>
	<s id="GROUP_LOGIN_MSG2">Enter the printer&apos;s current manager password.\nPrinter&apos;s that are already logged in are displayed with the unlocked icon.\nLogin all printers.</s>
	<s id="GROUP_LOGIN_MSG3">Password:</s>
	<s id="DLG_CAPTION_OPTION">Options</s>
	<s id="OPTION_TIMEOUT">Timeout</s>
	<s id="OPTION_COMMUNICATION_TIMEOUT">Time Before Declaring Communication Error (2-120):</s>
	<s id="OPTION_TIMEOUT_UNIT">seconds</s>
	<s id="OPTION_PROBE">Search Parameters</s>
	<s id="OPTION_PROBE_NETWORKADDRESS">Search with network address</s>
	<s id="OPTION_TCPIP_ADD_DLG_CAPTION">Add Search Address</s>
	<s id="OPTION_TCPIP_MCAST_ENABLE">Enable Search Using Multicast Packet</s>
	<s id="OPTION_TCPIP_ROUTING_ENABLE">Enable Search for a Network Outside the Router</s>
	<s id="OPTION_TCPIP_CAPTION_ROUTINGADDR">Search Address:</s>
	<s id="OPTION_TCPIP_NETWOKADDR">Network Address</s>
	<s id="OPTION_TCPIP_SUBNETMASK">Subnet Mask</s>
	<s id="OPTION_TCPIP_MCAST_TTL">Multicast TTL ($(MIN)-$(MAX)):</s>
	<s id="OPTION_TCPIP_CAPTION_NETWORK">Network Address:</s>
	<s id="OPTION_TCPIP_CAPTION_SUBNET">Subnet Mask:</s>
	<s id="OPTION_PROBE_IPADDRESS">Search with IP address</s>
	<s id="OPTION_PROBE_IPADDRESS_ENABLE">Enable search for the specified IP address</s>
	<s id="OPTION_LOG">Log</s>
	<s id="OPTION_LOG_GROUP">Log Output</s>
	<s id="OPTION_LOG_OUTPUT_ENABLE">Enable Log Output</s>
	<s id="OPTION_LOG_FILEPATH">Log File Path</s>
	<s id="OPTION_LOG_REF_DLG_TEXT">Select the log output destination.</s>
	<s id="OPTION_MSG_CONFIRM_RELOAD">You need to refresh the list to apply the settings.\nDo you want to refresh the list?</s>
	<s id="OPTION_MSG_CONFIRM_CANCEL_MODIFY">The setting information has been changed.\nIf you click [OK], all changes will be canceled.\nDo you want to continue?</s>
	<s id="OPTION_ERR_RANGE_INT">Enter an integer from $(MIN) to $(MAX).</s>
	<s id="OPTION_MSG_CONVERT">The network address $(INPUT) that you entered will be added to the list as $(OUTPUT) .\n</s>
	<s id="OPTION_MSG_REGISTERD">This address is already registered.</s>
	<s id="OPTION_MSG_CONFIRM_ADD_ADDR">Add this address?</s>
	<s id="OPTION_ERR_INVALID_ADDR">This address cannot be registered.</s>
	<s id="OPTION_ERR_CREATE_LOG">Cannot create a log file in the specified folder.</s>
	<s id="MB_CONFIRM_START">Proceed with the firmware update?</s>
	<s id="MB_CONFIRM_START_AUTOSHUTDOWN">Some of the printer(s) you selected come with a setting that turns the printer off automatically after a set amount of time.\nThe firmware update will fail if the printer is turned off during the update process.\nDo you want to disable this setting before starting the firmware update?</s>
	<s id="MB_CONFIRM_START_AUTOSHUTDOWN_DISABLE">The setting is restored before the firmware is updated.\nEnable the printer&apos;s Power Off Timer setting after completing the firmware update.</s>
	<s id="MB_CONFIRM_START_AUTOSHUTDOWN_ENABLE">Start the firmware update without restoring the setting.\nIf the printer is turned the power off during the update, the firmware will not be updated.</s>
	<s id="MB_CONFIRM_CANCEL">After the update for the printer currently being processed is complete, the update for the subsequent printer will be canceled.\nDo you want to continue?</s>
	<s id="MB_CONFIRM_CANCEL2">The firmware update for the following printer(s) will be canceled.\nDo you want to cancel it?</s>
	<s id="MB_CONFIRM_QUIT">Firmware update is not complete.\nAre you sure you want to exit?</s>
	<s id="MB_CONFIRM_CONTINUE">Are there any other printers/scanners that also need a firmware update?</s>
	<s id="MB_CONFIRM_MEASURE_WAITIDLE">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in use.\n- Ensure that the printer is not middle of the setup.</s>
	<s id="MB_CONFIRM_MEASURE_SENDING">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in use.\n- Ensure that the printer is not middle of the setup.\n\nBefore clicking [Retry], we recommend restarting the printer.</s>
	<s id="MB_CONFIRM_MEASURE_REBOOTPOLLING">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in recovery mode.\n\nIf you click [Retry] and the firmware update is failed, the printer is in recovery mode.</s>
	<s id="MB_CONFIRM_MEASURE_CHECKVERSION">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.</s>
	<s id="MB_CONFIRM_MEASURE_AUTOSHUTDOWN_DISABLE">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.</s>
	<s id="MB_CONFIRM_MEASURE_NOTFOUND">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.</s>
	<s id="MB_CONFIRM_LINK_DOWNLOAD">Epson Firmware Updater download site</s>
	<s id="MB_CONFIRM_MSG_DOWNLOAD">If the printer is in Recovery Mode, you will need to download the Firmware Updater file and manually install it.\nClick the link below to open a web page with instructions on downloading the file.\nExit this updater, then open the file you downloaded and follow the on-screen instructions.\n\nNote: Before opening the downloaded file, make sure your computer is connected to the printer with a USB cable. You cannot update the printer&apos;s firmware over a network connection when the printer is in recovery mode.</s>
	<s id="MB_CONFIRM_MSG_REBOOT">Finish the firmware update for all the printers and quit the running Epson Firmware Updater. Then, restart the Epson Firmware Updater and start updating by following the on-screen instructions.</s>
	<s id="MB_CONFIRM_VERSION_USBPREFIX">Start printer update.\n</s>
	<s id="MB_CONFIRM_VERSION_BASE">The printer has the following firmware.\n$(MESSAGE)\nDo you want to overwrite it?</s>
	<s id="MB_CONFIRM_VERSION_OLD">* This firmware is newer than the firmware file. \n</s>
	<s id="MB_CONFIRM_VERSION_SAME">* The firmware has already been updated.\n</s>
	<s id="MB_CONFIRM_VERSION_NODATA">* Cannot acquire version information.\n</s>
	<s id="TEXT_CONFIRM_1">Click [Retry] to perform the update again.\n</s>
	<s id="TEXT_CONFIRM_2">Click [Next] to continue processing.\n</s>
	<s id="TEXT_CONFIRM_3">Click [Stop] to cancel the following updates.\n</s>
	<s id="TEXT_CONFIRM_4">Click [Cancel] to exit.</s>
	<s id="TEXT_REBOOT_1">Reconnect the power supply for the updated printer.\nClick [Next] when the power is on.</s>
	<s id="TEXT_REBOOT_2">Confirm the firmware update is complete.\nReconnect the power supply for the updated printer after confirming the update.\nClick [Next] when the power is on.</s>
	<s id="TEXT_REBOOT_3">Address:</s>
	<s id="ERR_RUN_ALREADYRUNNING">Multiple programs cannot run simultaneously.</s>
	<s id="ERR_RUN_INVALID_OS">Cannot use under the current OS.</s>
	<s id="ERR_RUN_NO_STRING">Could not find files needed to start.</s>
	<s id="ERR_RUN_NO_SOCKET">Cannot launch the program.\nSocket initialization has failed.</s>
	<s id="ERR_RUN_NO_NETWORK">Cannot launch the program.\nA network protocol is not installed.</s>
	<s id="ERR_RUN_NO_RESOURCE">Cannot launch the program. \nIncorrect configuration file.</s>
	<s id="ERR_RUN_TEMPFOLDER_FAILED">Cannot launch the program. \nCould not create temporary folder.</s>
	<s id="ERR_RUN_UNKNOWN">Cannot launch the program.</s>
	<s id="ERR_OPEN_FORMAT">The firmware file is not correct.\nConfirm the firmware file, and then run this tool again.</s>
	<s id="ERR_OPEN_ALLOC">Not enough resources to proceed.</s>
	<s id="ERR_OPEN_BASE">The selected file is not a firmware file or the file may be corrupt.\nTry again after reselecting the firmware file or downloading the firmware file again.</s>
	<s id="ERR_OPEN_A2_UNKNOWN">Cannot use this type of firmware.</s>
	<s id="ERR_OPEN_ZCOUNT">\nThe number of Z sections is prohibited.</s>
	<s id="ERR_OPEN_UNSET">\nSection $(SECTION) key $(KEY) is not set.</s>
	<s id="ERR_OPEN_INVALID">\nSection $(SECTION) key $(KEY) is prohibited.</s>
	<s id="ERR_PASSWORD">Incorrect password.\nEnter the correct password.</s>
	<s id="ERR_INVALID_CHARACTER">Contains illegal characters.</s>
	<s id="ERR_INPUTLENGTH">Enter $(MIN) characters or more within $(MAX) characters.</s>
	<s id="ERR_DEVICELOCKED">Cannot set because it is locked.</s>
	<s id="ERR_DEVICEBUSY">Cannot set because the printer is busy.</s>
	<s id="ERR_IPLISTFILE">The IP Address List File is not correct. (error: $(LINE) line)\nConfirm the Internet Protocol address list file, and then run this tool again.</s>
	<s id="ERR_DISCONNECTED">The tool failed to communicate with the printer.\nCheck the printer&apos;s power supply and the cable connections.</s>
	<s id="ERR_NOTREADY">The printer is not ready to print.\nIf an error has occurred, clear the error.</s>
	<s id="ERR_PRINTFAILED">It has been failed to send the information on the current version.\nCheck the power supply and cable connection with the printer.</s>
	<s id="ERR_DOWNGRADE">Because the firmware is new, the printer cannot be updated.</s>
	<s id="ERR_CUSTOMFIRM">Because customer only firmware is applied to the connected printer, the printer cannot update the firmware.</s>
	<s id="ERR_NOTFOUND">The printer is not connected or the connected printer is not the target printer.</s>
	<s id="TITLE_NW_SEARCHING_SCANNER">Select the Scanner</s>
	<s id="TEXT_NW_SEARCHING_1_SCANNER">1. Under Model Name, select the scanner(s) you want to update.\n2. Click [Start] to begin updating.</s>
	<s id="TEXT_NW_FIREWALL_1_WIN1_SCANNER">Windows Firewall software will need to allow the Epson Firmware Updater to proceed with the update. Do you want to continue?\nIf you see a firewall warning message, click [Unblock] or [Allow] to let Epson Firmware Updater to continue.</s>
	<s id="STATE_UPDATE_AUTHENCATING_SCANNER">Confirming scanner password.</s>
	<s id="STATE_UPDATE_WAIT_IDLE_SCANNER">Scanner ready and standing by.</s>
	<s id="STATE_UPDATE_SENDING_SCANNER">Transmitting firmware file to the scanner.</s>
	<s id="STATE_UPDATE_WAIT_UPDATING_SCANNER">Firmware update in progress.</s>
	<s id="STATE_UPDATE_REBOOTPOLLING_SCANNER">Waiting for the scanner to restart.</s>
	<s id="STATE_UPDATE_CHECKVERSION_SCANNER">Firmware version confirmed.</s>
	<s id="STATE_SUCCEED_DEFAULT_SCANNER">The firmware update is complete.</s>
	<s id="STATE_SUCCEED_AUTOPOWEROFF_SCANNER">The firmware has been downloaded to your scanner.\nWait for the scanner to turn off automatically.</s>
	<s id="STATE_SUCCEED_EZ_AUTOPOWEROFF_SCANNER">The firmware has been downloaded to your scanner.\nWait for the scanner to turn off automatically. </s>
	<s id="STATE_SUCCEED_BIJ_RECOVERY_SCANNER">The firmware has been downloaded to your scanner.</s>
	<s id="STATE_FAILED_WAIT_IDLE_SCANNER">The scanner could not be updated.</s>
	<s id="STATE_FAILED_CAUSE_WAIT_IDLE_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off (disable the Power Off Timer setting in the scanner).\n- The scanner is busy.\n- A scanner error has occurred.</s>
	<s id="STATE_FAILED_SENDING_SCANNER">Failed to send the firmware file to the scanner.</s>
	<s id="STATE_FAILED_CAUSE_SENDING_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off (disable the Power Off Timer setting in the scanner).\n- The scanner is busy.\n- A scanner error has occurred.</s>
	<s id="STATE_FAILED_REBOOTPOLLING_SCANNER">Cannot confirm if the scanner has restarted.</s>
	<s id="STATE_FAILED_CAUSE_REBOOTPOLLING_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.\n- There was a loss of power to the scanner during the firmware update.</s>
	<s id="STATE_FAILED_CHECKVERSION_SCANNER">The scanner&apos;s firmware was not updated.</s>
	<s id="STATE_FAILED_CAUSE_CHECKVERSION_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.</s>
	<s id="STATE_FAILED_AUTOSHUTDOWN_SCANNER">- The scanner may have turned off if Power off Timer is enabled.</s>
	<s id="STATE_FAILED_AUTOSHUTDOWN_RESTORE_SCANNER">The Power Off Timer was not restored to its original setting.  </s>
	<s id="STATE_FAILED_AUTOSHUTDOWN_DISABLE_SCANNER">The scanner&apos;s Power Off Timer cannot be turned off.</s>
	<s id="STATE_FAILED_CAUSE_AUTOSHUTDOWN_DISABLE_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.</s>
	<s id="ERR_EZ_NOTFOUND_SCANNER">The scanner was not detected.</s>
	<s id="ERR_EZ_CAUSE_NOTFOUND_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.</s>
	<s id="ERR_EZ_NOTTARGET_SCANNER">The firmware has not been updated because it is not for the scanner connected.</s>
	<s id="STATE_WAITING_DETAIL_SCANNER">Waiting to complete update(s) for other scanner(s).</s>
	<s id="GROUP_LOGIN_SCANNER">Scanner Login</s>
	<s id="GROUP_LOGIN_MSG1_SCANNER">Enter the current administrator password.</s>
	<s id="GROUP_LOGIN_MSG2_SCANNER">Enter the scanner&apos;s current administrator password.\nScanner&apos;s that are already logged in are displayed with the unlocked icon.\nLogin all scanners.</s>
	<s id="MB_CONFIRM_START_SCANNER">Proceed with the firmware update?</s>
	<s id="MB_CONFIRM_START_AUTOSHUTDOWN_SCANNER">Some of the scanner(s) you selected come with a setting that turns the scanner off automatically after a set amount of time.\nThe firmware update will fail if the scanner is turned off during the update process.\nDo you want to disable this setting before starting the firmware update?</s>
	<s id="MB_CONFIRM_CANCEL_SCANNER">After the update for the scanner currently being processed is complete, the update for the next scanner will be canceled.\nDo you want to continue?</s>
	<s id="MB_CONFIRM_CANCEL2_SCANNER">The firmware update for the following scanner(s) will be canceled.\nDo you want to continue?</s>
	<s id="MB_CONFIRM_MEASURE_WAITIDLE_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is powered on.\n- Ensure that the scanner is not in use.\n- Ensure that the scanner is not in the middle of setting up.</s>
	<s id="MB_CONFIRM_MEASURE_SENDING_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is powered on.\n- Ensure that the scanner is not in use.\n- Ensure that the scanner is not in the middle of setting up.\n\nBefore clicking [Retry], we recommend restarting the scanner.</s>
	<s id="MB_CONFIRM_MEASURE_REBOOTPOLLING_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is powered on.\n\n</s>
	<s id="MB_CONFIRM_MEASURE_CHECKVERSION_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is on.</s>
	<s id="MB_CONFIRM_MEASURE_AUTOSHUTDOWN_DISABLE_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is on.</s>
	<s id="MB_CONFIRM_MEASURE_NOTFOUND_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is on.</s>
	<s id="MB_CONFIRM_MSG_DOWNLOAD_SCANNER">If the scanner is in Recovery Mode, you need to download the Firmware Updater file and install it manually.\nClick the link below to open a web page with instructions on downloading the file.\nExit this updater, and then open the file you downloaded and follow the on-screen instructions.\n\nNote: Before opening the downloaded file, make sure your computer is connected to the scanner with a USB cable. You cannot update the scanner&apos;s firmware over a network connection when the scanner is in recovery mode.</s>
	<s id="MB_CONFIRM_MSG_REBOOT_SCANNER">Finish the firmware update for all of the scanners, and then quit Epson Firmware Updater. Next, restart the Epson Firmware Updater and follow the on-screen instructions to start updating.</s>
	<s id="MB_CONFIRM_VERSION_USBPREFIX_SCANNER">Start scanner update.\n</s>
	<s id="MB_CONFIRM_VERSION_BASE_SCANNER">The scanner has the following firmware.\n$(MESSAGE)\nDo you want to overwrite it?</s>
	<s id="TEXT_REBOOT_1_SCANNER">Reconnect the power supply for the updated scanner.\nClick [Next] when the power is on.</s>
	<s id="TEXT_REBOOT_2_SCANNER">Confirm the firmware update is complete.\nReconnect the power supply for the updated scanner after confirming the update.\nClick [Next] when the power is on.</s>
	<s id="ERR_DEVICEBUSY_SCANNER">Cannot set because the scanner is busy.</s>
	<s id="ERR_DISCONNECTED_SCANNER">The tool failed to communicate with the scanner.\nCheck the scanner&apos;s power supply and the cable connections.</s>
	<s id="ERR_DOWNGRADE_SCANNER">Because the firmware is new, the scanner cannot be updated.</s>
	<s id="ERR_CUSTOMFIRM_SCANNER">Because customer only firmware is applied to the connected scanner, the scanner cannot update the firmware.</s>
	<s id="ERR_NOTFOUND_SCANNER">The scanner is not connected or the connected scanner is not the target scanner.</s>
	<s id="TEXT_UPDATE_5_SCANNER">Update Scanner List:</s>
	<s id="MB_CONFIRM_START_AUTOSHUTDOWN_DISABLE_SCANNER">Restore settings and then start the update.\nEnable the scanner&apos;s Power Off Timer setting after completing the firmware update.</s>
	<s id="MB_CONFIRM_START_AUTOSHUTDOWN_ENABLE_SCANNER">Start the firmware update without restoring settings.\nIf the scanner is turned off during the update, the firmware will not be updated.</s>
	<s id="MB_CONFIRM_SEARCH_SCANNER_MAC">Before updating the scanner&apos;s firmware, other applications that communicate with the scanner by USB need to be stopped. The next time you use the scanner, you need to log out and then login again.\nDo you want to stop other applications that are communicating with the scanner by USB?</s>
	<s id="MB_CONFIRM_CANCEL_SCANNER_MAC">The firmware update is not complete.\nThe next time you use the scanner, you need to log out and then login again.\nAre you sure you want to exit?</s>
	<s id="MB_CONFIRM_QUIT_SCANNER_MAC">The firmware file has been downloaded to your scanner.\nThe next time you use the scanner, you need to log out and then login again.\nAre you sure you want to exit?</s>
	<s id="COLUMN_MODELNAME_SERIAL">Model Name (Serial No.)</s>
	<s id="CHECK_SELECTFIRM">Select any software to update</s>
	<s id="ERR_LFP_DELETE_CHECK">It is strongly recommended that you select the update to keep your product up to date.\nAre you sure you want to deselect &quot;$(FIRMNAME)&quot; ?</s>
	<s id="ERR_LFP_DELETE_CHECK_UPDATE">Some updates are not selected. \nIt is strongly recommended that you select all firmware updates to keep your product up to date.\nDo you want to continue with the update?</s>
	<s id="ERR_LFP_NO_CONNECT">Firmware version information cannot be acquired.\n Please connect the &quot;$(FIRMNAME)&quot;, turn the printer off and on, and then click the [$(REFRESH)] button to try again.</s>
	<s id="ERR_LFP_NO_DATA">The selected update file does not contain all the data necessary for your configuration. Select an update file that includes data for $(FIRMNAME) if you wish to update all firmware.</s>
	<s id="STATE_FAILED_CAUSE_WAIT_IDLE_BATTERY">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off (disable the Power Off Timer setting in the printer).\n- The printer is busy.\n- A printer error has occurred.\n- The printer is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_REBOOTPOLLING_BATTERY">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.\n- There was a loss of power to the printer during the firmware update.\n- The printer is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_CHECKVERSION_BATTERY">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.\n- The printer is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_SENDING_BATTERY">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off (disable the Power Off Timer setting in the printer).\n- The printer is busy.\n- A printer error has occurred.\n- The printer is running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_WAITIDLE_BATTERY">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in use.\n- Ensure that the printer is not middle of the setup.\n- Ensure that the printer is not running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_SENDING_BATTERY">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in use.\n- Ensure that the printer is not middle of the setup.\n- Ensure that the printer is not running on the battery.\n\nBefore clicking [Retry], we recommend restarting the printer.</s>
	<s id="MB_CONFIRM_MEASURE_REBOOTPOLLING_BATTERY">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in recovery mode.\n- Ensure that the printer is not running on the battery.\n\nIf you click [Retry] and the firmware update is failed, the printer is in recovery mode.</s>
	<s id="MB_CONFIRM_MEASURE_CHECKVERSION_BATTERY">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_AUTOSHUTDOWN_DISABLE_BATTERY">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_NOTFOUND_BATTERY">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_WAIT_IDLE_ROLL">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off (disable the Power Off Timer setting in the printer).\n- The printer is busy.\n- A printer error has occurred.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="STATE_FAILED_CAUSE_REBOOTPOLLING_ROLL">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.\n- There was a loss of power to the printer during the firmware update.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="STATE_FAILED_CAUSE_CHECKVERSION_ROLL">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="STATE_FAILED_CAUSE_SENDING_ROLL">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or printer.\n- The Wi-Fi/Ethernet connection to your printer was lost.\n- The printer is powered off (disable the Power Off Timer setting in the printer).\n- The printer is busy.\n- A printer error has occurred.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="MB_CONFIRM_MEASURE_WAITIDLE_ROLL">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in use.\n- Ensure that the printer is not middle of the setup.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="MB_CONFIRM_MEASURE_SENDING_ROLL">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in use.\n- Ensure that the printer is not middle of the setup.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.\n\nBefore clicking [Retry], we recommend restarting the printer.</s>
	<s id="MB_CONFIRM_MEASURE_REBOOTPOLLING_ROLL">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- Ensure that the printer is not in recovery mode.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.\n\nIf you click [Retry] and the firmware update is failed, the printer is in recovery mode.</s>
	<s id="MB_CONFIRM_MEASURE_CHECKVERSION_ROLL">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="MB_CONFIRM_MEASURE_AUTOSHUTDOWN_DISABLE_ROLL">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="MB_CONFIRM_MEASURE_NOTFOUND_ROLL">The firmware update did not complete. Try the following, then click [Retry].\n- Ensure that the printer is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the printer is powered on.\n- For a printer with roll paper: If roll paper is loaded in the printer, remove it.</s>
	<s id="STATE_FAILED_CAUSE_WAIT_IDLE_BATTERY_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off (disable the Power Off Timer setting in the scanner).\n- The scanner is busy.\n- A scanner error has occurred.\n- The scanner is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_SENDING_BATTERY_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off (disable the Power Off Timer setting in the scanner).\n- The scanner is busy.\n- A scanner error has occurred.\n- The scanner is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_REBOOTPOLLING_BATTERY_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.\n- There was a loss of power to the scanner during the firmware update.\n- The scanner is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_CHECKVERSION_BATTERY_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.\n- The scanner is running on the battery.</s>
	<s id="STATE_FAILED_CAUSE_AUTOSHUTDOWN_DISABLE_BATTERY_SCANNER">The firmware update may have failed due to the following reason(s).\n- The USB cable is not connected to the computer or scanner.\n- The Wi-Fi/Ethernet connection to your scanner was lost.\n- The scanner is powered off.\n- The scanner is running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_WAITIDLE_BATTERY_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is powered on.\n- Ensure that the scanner is not in use.\n- Ensure that the scanner is not in the middle of setting up.\n- Ensure that the scanner is not running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_SENDING_BATTERY_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is powered on.\n- Ensure that the scanner is not in use.\n- Ensure that the scanner is not in the middle of setting up.\n- Ensure that the scanner is not running on the battery.\n\nBefore clicking [Retry], we recommend restarting the scanner.</s>
	<s id="MB_CONFIRM_MEASURE_REBOOTPOLLING_BATTERY_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is powered on.\n- Ensure that the scanner is not running on the battery.\n\n</s>
	<s id="MB_CONFIRM_MEASURE_CHECKVERSION_BATTERY_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is on.\n- Ensure that the scanner is not running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_AUTOSHUTDOWN_DISABLE_BATTERY_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is on.\n- Ensure that the scanner is not running on the battery.</s>
	<s id="MB_CONFIRM_MEASURE_NOTFOUND_BATTERY_SCANNER">The firmware update did not complete. Try the following, and then click [Retry].\n- Ensure that the scanner is connected (USB/Wi-Fi/Ethernet) to the computer.\n- Ensure that the scanner is on.\n- Ensure that the scanner is not running on the battery.</s>
</String>
